Your contact details
Company
Name:	Email:
Legal form:	Website:
Industry sector:	P.O. Box:
Street:	Zip code:
City:	Land:
VAT ID no.:	Other:
Person
Name:	Prename:
Department:	Position:
Email:	Mobile:
Telefone:	Telefax:
How do you come to us?
☐ Bayern International ☐ Recommendation ☐ Europages ☐ itsbetter.com ☐ Google ☐ LinkedIn ☐ Marktplatz Mittelstand ☐ Fair ☐ Wer Liefert Was ☐ XING ☐ Other: If recommended, who recommended us, please?
Why are you coming to us?
Reason for the search? ☐ Product optimization ☐ New product development
Reasons for changing supplier / product? ☐ Quality ☐ Price ☐ Service ☐ Compliance (Legal requirements) ☐ Supplier no longer exists ☐ Other:
☐ We are looking for a processor who coats our products with SEETHAN® We can establish this contact for you. ☐ We want to coat ourselves By completing this inquiry form, we can offer you the optimum SEETHAN® coating in terms of quality, price and processing for your individual area of application and the associated requirements.

Do you have the prerequisites for independent coating?
Compressed air	Spray room	Drying room (coated components)	Storage room (original containers)
☐ Compressor > 500 liters of air per minute	☐ Spray booth with turntable and lighting	☐ Storage possibility of the coated components	☐ Maintain a constant storage temp- erature of 20 °C
☐ Compressed air lines	☐ Explosion protection (ATEX)	☐ Explosion protection (ATEX)	☐ Comply with storage prohibitions with storage class 3
☐ Compressed air connections	☐ Extraction system	☐ Extraction system	☐ Sump trays available
☐ Compressed air tank as buffer storage	☐ Spray gun
☐ Refrigeration dryer	☐ Material pressure vessel
☐ Water separator
What equipment do you have for handling the containers?
Handling of 30 liter hobbocks: ☐ ATEX-certified agitator for mixing and stirring	Handling of 200 liter drums: ☐ ATEX-certified agitator for mixing and stirring ☐ ATEX-certified drum tipper ☐ ATEX-certified drum trolley ☐ 2“ Filling tap
Requirements Component
Carrier material	☐ PU-Foam ☐ PE-Foam ☐ Wood ☐ Metall ☐ Textile ☐ Other:	Surface area per component? [m2]
Processing condition of carrier material?	☐ Demolded ☐ Milled ☐ Sliced ☐ Other:	Previous / expected number of units per year?	☐ 1 - 10 ☐ 11 - 99 ☐ 100 - 999 ☐ 1.000 - 9.999 ☐ 10.000 - 99.999 ☐ 100.000 - 999.999 ☐ > 1.000.000
Geometry	☐ Flat surface that can be laminated with sheeting ☐ Free-form surface ☐ Deep bores, grooves, ... ☐ Other:	Gloss adjustment	☐ Glossy ☐ Satin matt ☐ Matt

Colors (See document „Color palette“)	☐ RAL ☐ PANTONE ☐ HKS	Can you provide us with sample parts for internal trials?	☐ Yes ☐ No
Can you provide us with a technical drawing?	☐ Yes ☐ No	Maximum service life in years?
Function and area of application of the component
Usage: ☐ Indoor use ☐ Outdoor use ☐ Visible component ☐ Invisible component	Adhesion: ☐ Permanent foil ☐ Removable foil	Place: ☐ Location (technical): ☐ Location (geographical):
Mechanical requirements
☐ Abrasion resistance: ☐ Load (static) ☐ Load (dynamic) ☐ Elongation at break [%]: ☐ Air tight ☐ Air permeable	☐ Maximum service life [years]: ☐ Minimum service life [years]: ☐ Shore-hardness: ☐ Water permeable ☐ Water tight
Chemical requirements
☐ Resistance to the following chemicals, solvents and cleaning agents: (See also document "Chemical resistance") ☐ Drying time, maximum [hours]:
Thermal requirements
☐ Temperature application range [°C] from: ☐ Temperature application range [°C] to: ☐ Flame retardant
Optical requirements
☐ Color fastness ☐ Surface (smooth) ☐ Surface (rough)	☐ Surface (single color) ☐ Surface (multicolored) ☐ Surface (structured)
Other requirements
☐ Resistance to X-rays ☐ Resistance to UV radiation ☐ Electrical conductivity	☐ Physiological harmlessness ☐ Environmental requirements: ☐ Certifications:
What parameters and framework conditions do we need to consider when selecting the right coating for you?